
SURREY SENSORS LTD. MD24HP-SERIES "HYDRA" RAKE TESTING EXECUTABLE

For use with version 1.x of the MD24HP-series digital probe rake system. Compatible with Win-10 systems. 

** Instructions for installation

(a) Ensure that you have installed the USB driver and any third-party drivers required. 

(b) Unzip this directory, and copy the directory in its entirety onto your computer.

(c) Double-click on the executables to run them- no further installation is necessary. 

(d) See user manual for specific instructions about linking calibration data, if pressure-to-velocity data conversion is desired. 

An example dataset is provided for testing purposes only, and to demonstrate the appropriate file formatting. Note that the sample data is configured for a single seven-hole probe head. 

** End user licence agreement

The installation and use of this software is subject to the Surrey Sensors Ltd. EULA, available at 

https://www.surreysensors.com/wp-content/uploads/2021/08/SD-EULA-100821.pdf